BlickP v1.4.1

Issues:

P122 L0 file on 2017.6.15 is empty (size = 0), this will cause BlickP stop working! But warning message is only check ICF or OF files.

Tips:

If want use new ICF file, need delete old ddf file in the calibration folder.

If want reprocess, need specify in config file that “froml1” or “froml2”, otherwise, L2 data will directly interpreted from L2fit, and no new L2fit will be made.